diff --git a/Tensile/Source/lib/source/hip/HipHardware.cpp b/Tensile/Source/lib/source/hip/HipHardware.cpp
index ffa4f0f..f894366 100644
--- a/Tensile/Source/lib/source/hip/HipHardware.cpp
+++ b/Tensile/Source/lib/source/hip/HipHardware.cpp
@@ -24,6 +24,8 @@
  *
  *******************************************************************************/
 
+#include <cstring>
+
 #include <Tensile/AMDGPU.hpp>
 #include <Tensile/hip/HipHardware.hpp>
 #include <Tensile/hip/HipUtils.hpp>
@@ -55,6 +57,20 @@ namespace Tensile
         {
             hipDeviceProp_t prop;
             HIP_CHECK_EXC(hipGetDeviceProperties(&prop, deviceId));
+            // coerce to compatible arch
+            int gcnArch = strncmp(prop.gcnArchName, "gfx", 3) == 0 ? std::stoi(prop.gcnArchName + 3) : 0;
+            switch(gcnArch)
+            {
+            case 902: case 909: case 912:
+                std::strcpy(prop.gcnArchName, "gfx900");
+                break;
+            case 1013:
+                std::strcpy(prop.gcnArchName, "gfx1010");
+                break;
+            case 1031: case 1032: case 1033: case 1034: case 1035: case 1036:
+                std::strcpy(prop.gcnArchName, "gfx1030");
+                break;
+            }
 #if HIP_VERSION >= 50220730
             int hip_version;
             HIP_CHECK_EXC(hipRuntimeGetVersion(&hip_version));
